## DL-40JANUS

## With or without an External Signal

## Source for Rescaling

0.56" or optional 0.8 large display red or green LED

General Features

External transmitters or signal conditioners can be eliminated

by directly connecting of the sensor output to one of Texmate's

29 Plug-in Input Signal Conditioners that include:

AC Current

AC/DC Voltage

Load Cell

Resistance

*Temperature

4 to 20 mA *See models DL-40-RTD and DL-40-RTD for higher accuracy

Pressure

Process

Prototype

digitally linearized thermocouple and RTD

Optional isolated 14 bit analog output. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired digital span from one count to the full scale range of 1999 to 9999 (12000 counts).

Optional Isolated Modbus RTU RS-485 serial communication with selectable baud rate (9600, 19200), address and parity.

Auto-sensing AC/DC power supply. For voltages between 85-265 VAC / 95-300 VDC (PS1) or 15-48 VAC / 10-72 VDC (PS2).

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors such as Load Cells and Pressure Transducers.

Standard red or optional green or super bright red 4-digit LED

display with range from 1999 to 9999 (12000 counts).

Red or green 0.8 LED large display option

Four annunciator LEDs provide front panel alarm status

indication for up to four setpoints.

Up to optional six relays in combination of six, four or two 4 Amp Form A relays or two 9 Amp Form C with two or four 4 Amp Form A relays are available.

Automatic intelligent averaging smooths noisy signals, while

providing a fast display response to real input signal changes.

Three-button programming via the front panel

(UP, DOWN and PROGRAM buttons).

Software Features

Front panel selectable four-level brightness control for digital

display and setpoint LEDs.

Four programmable setpoints.

Relay activation can be selected to occur above (HI) or below

(LO) each setpoint.

Hysteresis setting for all four setpoints. Delay on make and

delay on break for SP1 and SP2.

Peak and Valley. View and Reset.

Program Lock switch

A powerful, smart, programmable panel meter with optional Modbus RS-485 serial, analog and up to six relays output for measurement and control applications in a 1/8 DIN 96x48mm case.

Specifications

Input Specs:................Depends on Input signal conditioner A/D Converter:.............14 bit single slope Accuracy:.....................(0.05% of reading + 2 counts) Temp. Coeff.:...............100 ppm/C (Typical) Warm up time:.............2 minutes Conversion Rate:.........5 conversions per second (Typical) Display:........................4 digit 0.56" Red LED display (std),

0.56 or 0.8" Red, Green or Super Bright Red (optional)

Range 1999 to 9999 counts.

Polarity:........................Assumed positive. Displays negative Decimal Selection:.......Front panel button selectable, XXXX Positive Overrange:.....Top segments of digital display flash Negative Overrange:...Bottom segments of digital display flash Relay Output:..............Up to Six Relays in combination of six, four or two 4 Amp Form A relays or two

9 Amp Form C with two or four 4 Amp Form A relays.

Analog Output:............Isolated 14 bit user scalable mA or V AIC (mA out)................ 4-20 mA @ 0 to 500 max loop resis-

tance.

AIV (volts out).............. 0-10 V DC @ 500 or higher resistance Power Supply:.............AC/DC Auto sensing wide range supply PS1 (std)..................... 85-265 VAC / 95-300 VDC, 50-400Hz @ 3W PS2..............................15-48 VAC / 10-72 VDC, 50-400Hz @ 2.5W Operating Temp.:.........0 to 60 C Storage Temp:.............20 C to 70 C.

Relative Humidity:.......95% (non condensing) Case Dimensions:.......1/8 DIN, Bezel: 96x48 mm (3.78x1.89) Depth behind bezel: 117 mm (4.61) Plus 11.8 mm (0.47) for Right-angled

connectors, or plus 20 mm (0.79) for Straight-thru connector.

Weight:........................6.5 oz., 8.5 oz when packed

Input Module Compatibility

LEOPARD FAMILY: More than 29 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Leopard Family of meters.

Some examples are shown on pages 12 - 14.

See www.texmate.com for an up to date listing.

### Index

Page 1

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.