Center Bar

for Dual Scale

Applications

(Tri-Color or

Mono-Color)

LEOPARD FAMILY

## FL-B101Q

## Leopard Bargraph Meter

## 101 Segment LEDs

## in a 9/64 DIN CASE

### Smart mono-color digital bargraph

### with four fully programmable set points for

### monitoring, measurement, and control applications.

Left or Right Bar to match 6 Edgewise Mechanical Meters with Left or Right Pointers (Mono-Color only)

### General Features

Two 9 Amp Form C, and two 4 Amp Form A relays available

Auto-sensing AC/DC power supply. For voltages between 85-265 V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

Optional isolated 16 bit analog output. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired span from one bar to the full scale range

Provision to connect an external programming lockout switch.

Optional NEMA-4 front cover.

24 V DC excitation is available to power external 4/20 mA transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors.

UL Listed

Software Features

The two 101 segment bargraph can be independently scaled.

Bargraph center zero function.

Four programmable setpoints.

Relays activation can be selected to occur above (HI) or below (LO)

each setpoint.

Decimal point setting.

### Input Module Compatibility

LEOPARD FAMILY: More than 50 different Plug-in I-Series Input Signal Conditioners are approved for Leopard Family meters.

Specifications

Input Specs:..............Depends on range and function selected A/D Converter:..........14 bit single slope Accuracy:..................(0.05% of reading + 1segment) Temp. Coeff.:.............100 ppm/C (Typical) Warm up time:...........2 minutes Conversion Rate:......10 conversions per second (Typical) Bargraph Display:.....101 segment 4 vertical

(std), horizontal (optn), red (std), green (optn), one red one green (optn)

Polarity:.....................Selectable center zero Positive Overrange:..Bargraph display flashes Negative Overrange: First segment of bargraph display flashes Relay Output:............Two 4 Amp Form A relays and Two

9 Amp Form C relays

Analog Output:.........Isolated 16 bit user scalable mA or V

OIC

OIV

(mAout)...........4-20 mA @ 0 to 500 max loop resistance (volts out).......... 0-10 V DC @ 500 or higher resistance Power Supply:...........AC/DC Auto sensing wide range supply PS1 (std)................85-265 VAC, 50-400 Hz / 95-300 VDC @ 4.2W PS2...................... 15-48 VAC,50-400 Hz / 10-72 VDC @ 4.2W Operating Temp.:......0 to 50C Storage Temp:...........20C to 70C Relative Humidity:....95% (non condensing) Case Dimensions:....3/32 DIN, Bezel: 36x144 mm(1.42x5.69) Depth behind bezel: (4.64") 117.5 mm Plus 10 mm (0.39) for Right-angled connector, or plus 18.3 mm (0.72) for Straightthru connector, or plus 26.5 mm (1.05) for Push-On connector.

Weight:.......................9.5 oz., 12 oz when packed

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.