## DX-35

## Lynx Panel Meter

## 3 1/2 DIGIT 0.56 or 0.8 L ED

## in a 1/8 DIN Case

LYNX FAMILY

### A versatile digital panel meter with standard or large

### display, for monitoring and measurement applications.

Large display option

0.8 red or green LED

E469078

General Features

External transmitters or signal conditioners can be eliminated by directly connecting the sensor to more than 33 I-Series Plug-in Input Signal Conditioners that include:

AC Current

AC Voltage

DC Current

DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Strain-gage

Temperature

4 to 20 mA

Pre-calibrated I-Series Input Signal Conditioning modules, that

have span or zero potentiometers, can be interchanged between any I-Series compatible meter, without recalibration, because all of the analog scaling and reference circuitry is self-contained within the module.

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for strain-gages, load cells and resistance bridge type sensors.

AC/DC Auto-sensing power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

Standard red or optional green or super bright red 3 1/2-digit 0.56

LED with display range 1999 to 1999 (4000 counts).

Red or green 0.8" LED large display option.

Display brightness may be externally controlled.

1/8 DIN (96 x 48mm ) case easily mounts in thin or thick panels (up to 2). May be ordered with optional extra fire resistant metal case.

Optional NEMA-4X, IP-65 hinged, lockable, water and dust

proof cover.

UL Listed

### Input Module Compatibility

LYNX FAMILY: More than 33 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Lynx Family of meters.

See www.texmate.com for an up to date listing.

### Specifications

Input Specs:..............Depends on input signal conditioner A/D Converter:..........12 bit dual slope Accuracy:..................(0.05% of reading + 2 counts) Temp. Coeff.:............100 ppm/C (Typical) Warm up time:..........2 minutes Conversion Rate:......3 conversions per second (Typical) Display:......................3 1/2 digit 0.56" Red LED display (std),

0.56 or 0.8 Green or Super Bright Red (optn). Range 1999 to 1999 counts.

Polarity:....................Assumed positive. Displays negative Decimal Selection:....Header under face plate, XXXX Positive Overrange:..1 (MSD) is displayed with all other digits blank.

Negative Overrange: 1 (MSD) and sign are displayed with

all other digits blank.

Power Supply:..........AC/DC Auto sensing wide range supply PS1 (std)................85-265 VAC, 50-400Hz / 95-300 VDC @ 1.5W PS2........................15-48 VAC, 50-400Hz / 10-72 VDC @ 4.0W

Operating Temp.:......0 to 50 C Storage Temp:..........20 C to 70 C.

Relative Humidity:....95% (non condensing) Case Dimensions:....1/8 DIN, Bezel: 96x48 mm (3.78"x1.89")

Depth behind bezel: 117 mm (4.61") Plus 11.8 mm (0.47") for Right-angled connector or plus 20 mm (0.79") for Straight-thru connector.

Weight:......................8 oz., 11 oz when packed.

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.