LYNX FAMILY

## BX-B31

## Lynx Bargraph Meter

## 31 LED Segments

## in a 1/16 DIN Case

A versatile, modular bargraph with optional single or dual setpoints.

### General Features

31 segment AC/DC powered modular compact bargraph.

1/16 DIN (96 x 24mm ) case easily mounts in thin or thick panels (up to 2).

Red (std), green (optional) or amber (optional) colors.

Vertical or horizontal formats.

External transmitters or signal conditioners can be eliminated by directly connecting the sensor to more than 33 I-Series Plug-in Input Signal Conditioning Modules that include:

AC Current

AC Voltage

DC Current

DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Strain-gage

Temperature

4 to 20 mA

Pre-calibrated I-Series Input Signal Conditioning modules, that have span or zero potentiometers, can be interchanged between any I-Series compatible meter, without recalibration, because all of the analog scaling and reference circuitry is self-contained within the module.

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for strain-gages, load cells and resistance bridge type sensors.

High voltage power supply (PS1) 85 - 265VAC / 95 - 300VDC Low voltage power supply (PS2) 15 - 48VAC / 10 - 72VDC

Optional single or dual setpoints with easy adjustment

from the front.

Dual 4A Form A relays or one 4A Form A and one 9A

Form C relays.

Easy configuration of relays as high or low setpoints.

Proportional brightness mode for increased effective opti-

cal resolution.

UL Listed.

### Input Module Compatibility

LYNX FAMILY: More than 33 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Lynx Family of meters.

See www.texmate.com for an up to date listing.

Specifications

Input Specs:..............Depends on input signal conditioner

A/D Converter:..........31 step flash converter

Accuracy:..................(0.05% of reading + 3 counts)

Temp. Coeff.:............100 ppm/C (Typical)

Warm up time:..........2 minutes

Display:......................Thirty-one 0.2 x 0.06 (5.08 x 1.52mm)

LED segments. Red display (std), green

(opt) or amber (opt)

Positive Overrange:..All segments flash.

Negative Overrange:..Zero segment flashes

Power Supply:..........AC/DC Auto sensing wide range supply

PS1 (std)................85-265 VAC, 50-400Hz / 95-300 VDC @ 1.5W

PS2........................15-48 VAC, 50-400Hz / 10-72 VDC @ 4.0W

Operating Temp.:......0 to 50 C

Storage Temp:..........-20 C to +70 C

Relative Humidity:....95% (non condensing)

Case Dimensions:....1/16 DIN, Bezel: 96x24mm(3.78x0.95)

Depth behind bezel 122.2 mm (4.83")

Plus 12.7mm (0.5) for Right-angled

connector.

Weight:......................198 gms (7 oz)

255 gms (9 oz) when packed

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.