## DI-50EB51H & DI-50TB51H

## Programmable Meter Controllers

## Tiger 320 Series PMCs

## 51 Segment Bargraph, 5 Digit 0.31 LEDs

## in a 1/8 DIN Case

### A powerful, intelligent, 5-digit, 51-segment Programmable

### Meter Controller (PMC) with modular outputs, input signal

### conditioning and advanced software features for monitoring,

### measurement, control and communication applications.

General Features

The Tiger 320 Operating System supports an easy to use PC based Configuration Utility Program, which can be downloaded FREE from the web, and programming from front panel buttons.

The T Version supports custom macro programs that can be easily produced with the Tiger 320 Macro Development System (available FREE on the web). The Development System enables programs to be written in BASIC, which can utilize any combination of the hundreds of functions and thousands of registers embedded in the Tiger 320 Operating System.

Red or green 7-segment, 0.31 high LEDs with full support

for seven segment alphanumeric text.

Brightness control of LED display from front panel buttons.

51 segment red or green bargraph that can display the signal from any of four channels or the result of a processed input signal.

Modular construction with more than 120 interchangeable input signal conditioners and more than 25 interchangeable I/O modules.

Up to 4 input channels with cross channel math for multi-

channel processing.

For applications where sensor excitation is required, modules are provided with 5V, 10V or 24 V DC voltage outputs.

On demand tare, calibration and compensation can be initi-

ated by the front panel program button.

Autozero maintenance for super stable zero reading is pro-

vided for use in weighing applications.

Programmable input averaging and smart digital filtering for

quick response to input signal changes.

Display text editing. Customize display text for OEM applica-

tions.

Scrolling display text messaging on T meters with macros.

Auto-sensing high voltage or optional low voltage AC / DC

power supply.

Serial output options include RS-232, RS-485, ModBus, Ethernet, DeviceNet or direct meter-to-meter communications.

Single or dual 16-bit Isolated Analog Outputs. Programmable 0~4 to 20mA or 0 to 10V for retransmission, 4-20mA loops to drive valve actuators, remote controllers & displays, multiloop feedback and PID output. Scalable from 1 count to full scale.

Dual independent totalizers to integrate input signals.

6 super smart, independently programmable setpoints with 8 selectable functions, including latching, deviation, hysteresis, register resetting, tracking and dual PID. Plus 7 programmable timer modes on all 6 setpoints.

Setpoint tracking, setpoint latching and manual relay reset.

Setpoints activated from any input, any register in the meter

or from any digital input.

Plug-in I/O modules include electromechanical or solid state relays, logic outputs or open collector outputs. 6 inputs & 16 outputs of opto-isolated I/O can be connected to an external DIN Rail terminal block module.

Internal program safety lockout switch to prevent tampering.

Peak & valley (max & min) with front panel recall and reset.

Real time clock with 15 year Lithium battery backup.

Data logging within the meter (up to 4000 samples with date/

time stamp).

Optional NEMA-4 front cover.

Input Module Compatibility

TIGER FAMILY: More than 120 different Plug-in I-Series Input Signal Conditioners are approved for the Tiger Family of meters.

See I-Series Input Signal Conditioning Modules Guide (Z87) for an up-to-date list.

General Features................... 1 Specifications....................... 2 Tiger 320 Series Literature Overview... 3 Tiger 320 Series System Overview... 4-5 Planning to Use the Tiger 320....... 6-8 Block Diagram of Tiger 320 Structure... 9 Configuration Utility Program......... 10 Custom Macro Program............. 11 Index......................... 12-13

Table of Contents

Controls & Indicators............. 14-15 Front Panel Configuration & Setup..... 16 Front Panel Programming Codes... 17-18 Initial Setup Procedures.......... 19-20 Display Brightness.................. 20 Calibration Modes............... 21-24 Programming Procedures......... 25-41 Setpoint Programming Mode...... 42-47 Registers......................... 48

Functional Diagram................. 49 Connector Pinouts.................. 49 Carrier Board Output Pins........... 50 Relay and Logic I/O Modules......... 50 Component Layout & Ext. Devices... 51-52 I-Series Input Modules........... 53-59 Ordering Information............. 60-62 Custom Faceplates................. 63 Case Dimensions.................. 64

DI-50EB51H&DI-50TB51H (d0041)

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

Page 1

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.