# CL-B101D40

### Smart 101 segment, 4 digit LED Tricolor or Mono-

### color digital bargraph controller with

### four fully programmable set points

### in a switchboard style case for

### monitoring, measurement, and control applications.

0.56 LEDs

General Features

External transmitters or signal conditioners can be eliminated by

Specifications

Input Specs: Depends on Input signal conditioner A/D Converter: 14 bit single slope Accuracy: (005% of reading + 2 counts) Temp. Coeff: 100 ppm/C (Typical) Warm up time: 2 minutes Conversion Rate: 10 conversions per second (Typical) Digital Display: 4 digit 0.56" LED red (std), green (optn)

Range 1999 to 9999 counts

Bargraph Display: 101 segment 235o circular red (standard),

Green (optional) or tricolor (optional) LED

Polarity: Assumed positive Displays negative Decimal Selection: Front panel button selectable, XXXX Positive Overrange: Bargraph and top segments of digital display

flash

Negative Overrange: First segment of bargraph and bottom seg-

ments of digital display flash

Relay Output: Two 9 Amp Form C relays, two 4 Amp Form

A relays or 4 x 4 Amp Form A relays

Analog Output: Isolated 16 bit user scalable mA or V OIC (mA out) 4-20 mA @ 0 to 500 max loop resistance OIV (volts out) 0-10 V DC @ 500 or higher resistance Power Supply: AC/DC Auto sensing wide range supply PS1 (std) 85-265 VAC / 95-300 VDC, 50-400Hz 4.2W PS2 18-48 VAC / 10-72 VDC, 50-400Hz 42W Operating Temp: 0 to 50C Storage Temp: 20C to 70C Relative Humidity: 95% (non condensing) Case Dimensions: Bezel (4.48"x4.48") 113.8x113.8mm

Depth behind bezel (4.23") 107.46 mm Plus (048) 1224 mm for connectors

Weight: 16 oz, 1lb 4 oz when packed

direct connection of the sensor output to more than

40 Plug-in Input Signal Conditioners that include:

AC/DC Current

AC/DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Temperature

4 to 20 mA

Optional isolated 16 bit analog output. User or factory scalable to 4

to 20 mA, 0 to 20 mA or 0 to 10 V across any desired digital span from one count to the full scale range of 1999 to 9999 (12000 counts).

A Programmable Tricolor (Red-Green-Orange) or mono color (red or

green), 101 segment high brightness bargraph.

Red 4-digit LED display with a range of -1999 to 9999

(12000 counts). Optional green digital display.

Front panel LED annunciators provide indication of setpoint status.

Two 9 Amp Form C, and two 4 Amp Form A or 4 x 4 Amp Form A relays available.

Auto-sensing AC/DC power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 18-48 V AC / 10-72 V DC (PS2).

24 V DC excitation is available to power external 4/20mA transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors.

Provision to connect an external programming lockout switch.

Provision for external DIM switch to reduce the brightest

display setting by 50%.

Automatic intelligent averaging, smooths noisy signals while providing a fast display response to real level changes.

Software Features

The bargraph can display, full scale, any desired portion of the digital reading.

Setpoint 1 has delay-on-make

and delay-on-break plus

a special pump on pump off mode that creates a Hysteresis Band between SP1 and SP2.

Four programmable setpoints with adjustable Hysteresis.

Bargraph center zero function.

Relay activation can be selected to occur above (hi) or below

(Lo) each setpoint.

Digital display blanking.

Decimal point setting.

Four-level brightness control

Bargraph Center Point Display Mode Selection... 6 Bargraph Color Programming Mode........ 9 Case Dimensions....................... 7 Component Layout..................... 11 Connector Pinouts..................... 10 Connectors........................... 11 Controls and Indicators.................. 2 Decimal Point and Brightness Selection..... 5

Table of Contents

Digital Span Selection for Display.......... 5 Digital Span Selection for Analog Range Output... 6 Functional Diagram.................... 10 General Features....................... 1 I-Series Input Signal Conditioning Modules... 12-14 Input Module Calibration Procedures...... 16 Input Module Component Glossary........ 15 Installation guidelines................... 17 Ordering Information................... 18

Pin Descriptions....................... 10 Programming Conventions................ 2 Setpoint Setting & Relay Configuration Mode.... 8-9 Software Features...................... 1 Software Logic Tree..................... 3 Specifications.......................... 1 Two Point Analog Range Setting & Calibration.... 7 Two Point Digital Calibration Mode......... 4

Page 1

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.