## BX-35

## Lynx Panel Meter

## 3 1/2 DIGIT 0.56 L ED

## in a 1/16 DI N Case

LYNX FAMILY

A versatile panel meter that utilizes many different types of modular plug-in signal conditioners.

### General Features

### Input Module Compatibility

External transmitters or signal conditioners can be eliminated

by directly connecting the sensor to more than 33 I-Series

Plug-in Input Signal Conditioning Modules that include:

LYNX FAMILY: More than 33 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Lynx Family of meters.

AC Current

AC Voltage

DC Current

DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Strain-gage

Temperature

4 to 20 mA

Pre-calibrated I-Series Input Signal Conditioning modules, that

have span or zero potentiometers, can be interchanged between

any I-Series compatible meter, without recalibration, because all

of the analog scaling and reference circuitry is self-contained with-

in the module.

24 V DC excitation is available to power external transmitters

and 5 or 10 V DC excitation is available for strain-gages, load

cells and resistance bridge type sensors.

Auto-sensing AC/DC power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

Standard red or optional green or super bright red 3 1/2-digit

0.56 LED with display range 1999 to 1999 (4000 counts).

Display brightness may be externally controlled

1/16 DIN (96 x 24mm ) case easily mounts in thin or thick

panels (up to 2).

UL Listed

See www.texmate.com for an up to date listing.

### Specifications

Input Specs:..............Depends on input signal conditioner A/D Converter:..........12 bit dual slope Accuracy:..................(0.05% of reading + 2 counts) Temp. Coeff.:............100 ppm/C (Typical) Warm up time:..........2 minutes Conversion Rate:......3 conversions per second (Typical) Display:......................3 1/2 digit 0.56" Red LED display (std), 0.56 Green or Super Bright Red (optn).

Range 1999 to 1999 counts.

Polarity:....................Assumed positive. Displays negative Decimal Selection:....Header under face plate, XXXX Positive Overrange:..1 (MSD) is displayed with all other dig-

its blank.

Negative Overrange: 1 (MSD) and sign are displayed with

all other digits blank.

Power Supply:..........AC/DC Auto sensing wide range supply PS1 (std)................85-265 VAC, 50-400Hz / 95-300 VDC @ 1.5W PS2........................15-48 VAC, 50-400Hz / 10-72 VDC @ 4.0W

Operating Temp.:......0 to 50 C Storage Temp:..........20 C to 70 C.

Relative Humidity:....95% (non condensing) Case Dimensions:....1/16 DIN Bezel: 96x24mm (3.78x0.95)

Depth behind bezel 122.2 mm (4.83") Plus 12.7mm (0.5) for Right-angled connector.

Weight:......................7 oz., 9 oz when packed

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.