## DX-40

## Lynx Panel Meter

## 4 DIGIT0.8 LED

## DX-45

## Lynx Panel Meter

## 4 1/2 DIGIT 0.56 LED

## Both in a 1/8 DIN Case

LYNX FAMILY

### A versatile, standard and large display, series of digital

### panel meter for monitoring and measurement applications.

Large display DX-40

0.8 red or green LED

E469078

General Features

External transmitters or signal conditioners can be eliminated by directly connecting the sensor to more than 33 I-Series Plug-in Input Signal Conditioners that include:

AC Current

AC Voltage

DC Current

DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Strain-gage

Temperature

4 to 20 mA

Precalibrated I-Series input modules, that have span or zero potentiometers, can be interchanged between any I-Series compatible meter, without recalibration, because all of the analog scaling and reference circuitry is self-contained within the module.

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for straingages, load cells and resistance bridge type sensors.

Auto-sensing AC/DC power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

Standard red or optional green or super bright red 4 1/2digit 0.56" LED with display range 19999 to 19999 (40000 counts DX-45).

Display brightness may be externally controlled.

Standard red or optional green 4-digit 0.8" LED with display range -9999 to 9999 (20000 counts DX-40).

Optional NEMA-4X, IP-65 hinged, lockable, water and dust

proof cover.

1/8 DIN (96 x 48mm ) case easily mounts in thin or thick panels (up to 2). May be ordered with optional extra fire resistant metal case.

UL Listed

Input Module Compatibility

LYNX FAMILY: More than 33 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Lynx Family of meters.

See www.texmate.com for an up to date listing.

### Specifications

Input Specs:..............Depends on input signal conditioner A/D Converter:..........16 bit dual slope Accuracy:..................(0.05% of reading + 3 counts) Temp. Coeff.:............100 ppm/C (Typical) Warm up time:..........2 minutes Conversion Rate:......3 conversions per second (Typical) Display:....DX-45......4 1/2 digit 0.56 Red LED display (std) 0.56 Green or Super Bright Red (optn).

Range 19999 to 19999 counts.

DX-40......4 digit 0.8 Red LED display (std)

0.8 Green (optn).

Range 9999 to 9999 counts.

Polarity:....................Assumed positive. Displays negative Decimal Selection:....Header under face plate DX-45......XXXXX

DX-40......XXXX

Positive Overrange:..All digits flash.

Negative Overrange: negative sign and all digits flash Power Supply:..........AC/DC Auto sensing wide range supply 85-265 VAC, 50-400Hz / 95-300 VDC @ 1.5W 15-48 VAC, 50-400Hz / 10-72 VDC @ 1.5W

PS1 (std)................

PS2........................

Operating Temp.:......0 to 50 C Storage Temp:..........20 C to 50 C.

Relative Humidity:....95% (non condensing) Case Dimensions:....1/8 DIN, Bezel: 96x48 mm (3.78"x1.89")

Depth behind bezel: 117 mm (4.61") Plus 11.8 mm (0.47") for Right-angled connector or plus 20 mm (0.79") for Straight-thru connector.

Weight:......................8 oz., 11 oz when packed.

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.