E469078

## FX-B101Q

## Lynx Bargraph Meter

## 101 Segment

## in a 9/64 DIN CASE

LYNX FAMILY

### A low cost red or optional green, 101 segment bargraph in a 36x144 case, providing

### a direct connection to most sensors for monitoring and measurement applications.

General Features

External transmitters or signal conditioners can be eliminated by directly connecting the sensor to more than 33 I-Series Plug-in Input Signal Conditioning Modules that include:

AC Current

AC Voltage

DC Current

DC Voltage

Load Cell

Pressure

Process

Prototype

Resistance

Strain-gage

Temperature

4 to 20 mA

Pre-calibrated I-Series Input Signal Conditioning modules, that have span or zero potentiometers, can be interchanged between any I-Series compatible meter, without recalibration, because all of the analog scaling and reference circuitry is self-contained within the module. 5 or 10 V DC excitation is provided for resistance bridge type sensors.

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for strain-gages, load cells and resistance bridge type sensors.

A red or optional green 101 segment bargraph.

Auto-sensing AC/DC power supply. For voltages between 85-265 V AC / 95-300 V DC (PS1) or 14-48 V AC / 10-72 V DC (PS2).

Optional 16 Bit isolated analog output that can be used to drive an external process device such as a chart recorder, remote display, or for retransmission to a central control room. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired span from one bar to the full scale range

Center zero setting, header selectable.

Provision for external brightness setting switch (by connecting the DIM to the GND pin on the back of the meter).

Smart averaging (to speed up display response).

Optional NEMA-4 front cover.

UL Listed

### Input Module Compatibility

LYNX FAMILY: More than 33 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Lynx Family of meters.

See www.texmate.com for an up to date listing.

### Specifications

Input Specs:..............Depends on range and function selected A/D Converter:..........14 bit single slope Accuracy:..................(0.05% of reading + 1segment) Temp. Coeff.:.............100 ppm/C (Typical) Warm up time:...........2 minutes Conversion Rate:......10 conversions per second (Typical) Bargraph Display:.....101 segment 4 vertical (std),

horizontal (optn), red (std), green (optn)

Polarity:.....................Selectable center zero Positive Overrange:..Bargraph display flashes Negative Overrange: First segment of bargraph display flashes Analog Output:.........Isolated 16 bit user scalable mA or V OIC (mA out)...........4-20 mA @ 0 to 500 max loop resistance OIV (volts out)......... 0-10 V DC @ 500 or higher resistance Power Supply:...........AC/DC Auto sensing wide range supply PS1 (std)..................85-265 VAC, 50-400Hz / 95-300 VDC @ 1.5W PS2...............................14-48 V AC, 50-400Hz / 10-72 V DC @1.5W Operating Temp.:......0 to 50C Storage Temp:...........20C to 70C Relative Humidity:....95% (non condensing) Case Dimensions:....3/32 DIN, Bezel: 36x144 mm(1.42x5.69) Depth behind bezel: (4.64") 117.5 mm Plus 10 mm (0.39) for Right-angled connector, or plus 18.3 mm (0.72) for Straightthru connector, or plus 26.5 mm (1.05) for Push-On connector.

Weight:.......................9.5 oz., 12 oz when packed

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.