# 16-BIT SMART DUAL LOAD CELL MODULE

## Fits Tiger 320 Series

Crystal

Controlled 50/60 Hz

Noise Rejection option.

On-board Excitation

Voltage Generator.

Enough to power 8 x 350 bridges.

Interface to

Tiger Meter.

State-of-the-art

Electromagnetic Noise

Suppression Circuitry.

Ensures signal integrity under harsh EMC environments.

8-pin Input

Connector.

Dual load cell and excitation.

On-board Digital Signal

Processor.

Provides output rates, selectable gains and digital filtering

for dual load cell inputs.

Ultra-low noise 16-bit

A/D Convertor.

Approaches 19-bit performance

with additional software filtering.

6-wire or 4-wire Bridge Header selectable.

The revo lution in intelligent loa d c el l c o ntr ol l e rs co nti n u es wi t h our du al i n put modu l e.

This powerful input module defines the next generation of intelligent load cell controllers, encapsulating high performance and precision measurement with dual input functionality.

When combined with the Tiger 320 Series operating system, the operator has all the solutions to weighing, bagging and continuous batching control applications. All these features plus the bonus of dual load cell inputs make this module the obvious choice over dated weighing controllers, PLC and timer technology.

Input Module

Order Code Suffix

Excitation

Input Range

Input Channels

Input Sensitivity

Zero Drift

Span Drift

Non-linearity

Input Noise

Signal Processing Rate

Frequency Select

Hardware Module Specifications

5 V DC, 130 mA maximum.

Software selectable for sensors from 1 mV/V to 20 mV/V.

Dual, independent gains. Zero X-talk between channels each having 19-bit effective resolution.

0.08 V/Count maximum.

40 nV/ C typical. 200 ppm/ C of full scale maximum. 0.003% of full scale maximum.

160 nVp-p typical at 1 Hz output rate.

20 Hz maximum, 1 Hz minimum.

50/60 Hz noise rejection.

Output Rates

Gain Select

Software Module Features

A choice of average response outputs, 1-20 Hz.

Choice of industry standards, 1-20 mV/V.

Frequency Select

50/60 Hz noise rejection.

Some Relevant Tiger 320 Series Operating System Features

ISS5-6 Data Sheet (NZ328)

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

Page 1

### Programming Quick Start Guide

Smart Setup Registers

The meter uses three smar t setup registers to configure smart input modules. ISS5 and ISS6 require smart registers 1 and 2 to be set up. Because this is a dual input module, independent sensor inputs can be softw are selected for channels 1, 2, 3, and 4.

Sensor 1 and/or sensor 2 can be transferred to Channel

1 via Code 2, to Channel 2 via Code 4, to Channel 3 via Code 5, and to Channel 4 via Code 6.

### Connector Pinouts

### Programming Procedures

Press the

and

buttons at the same time to enter the main prog ramming mode.

Press the

button three times to enter Code 2. Set Code 2 to [X77].

Note the output register map is different for each smart input module.

This setting enters the smart register 1 code setup menu.

Press the

button.

This men u pro vides settings unique to smart register 1 of input module ISS5.

Using the

sensor 1 input, and the output rate common to both sensor inputs.

buttons, select the rele vant line frequenc y rejection,

5 Press the

button. The display returns to [Cod_2] [X77].

6 Using the

button, reset the 3rd digit to z ero [X70] to leave the smart register 1 menu.

Note, leaving the 3rd digit as 7 means the displa y constantly cycles between [Cod_2] and [SMt1].

Press the

button 3 times to enter Code 5. Set Code 5 to [X77].

Note the output register map is diff erent f or eac h smar t input module.

Page 2

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

ISS5-6 Data Sheet (NZ328)

Press the

button.

This setting enters the smart register 2 code setup menu.

This men u pro vides settings unique to smart register 2 of the ISS5 and ISS6 input module.

Using the

buttons, select the sensor 2 input from the 3rd digit.

Press the

button to save the settings.

The display toggles between [Cod_5] and [X77].

Using the

button, reset the 3rd digit to 0 to lea ve the smart register 2 menu.

Press the

and

button at the same time to retur n to the operational display.

## Select a Channel

Select the output register for the required channels

Press the

and

button at the same time again to re-enter the main prog ramming mode.

Press the

button three times to enter Code 2.

Set Code 2 to [X7X]. Select the required processing rate for CH1 in the 1st digit and the required register map settings (sensor 1 or sensor 2) in the 3rd digit.

## CH1

Note the output register map is different for each smart input module type.

If required enter Code 4 and select the required register map settings f or CH2 in the 2nd digit.

## CH2

If required enter Code 5 and select the required post processing settings f or CH3 in the 1st digit and the required register map settings in the 3rd digit.

## CH3

From Procedure 18, page 4

Note the output register map is different for each smart input module type.

ISS5-6 Data Sheet (NZ328)

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

Page 3

If required enter Code 6 and select the required post processing settings f or CH4 in the 1st digit and the required register map settings in the 3rd digit.

## CH4

Press the

button to save the settings.

Press the

time to return to the operational display.

buttons at the same

and

To Procedure 17, page 3

### Customer Configuration Settings:

1st Digit

2nd Digit 3rd Digit

1st Digit

2nd Digit 3rd Digit

1st Digit

2nd Digit 3rd Digit

1st Digit

2nd Digit 3rd Digit

1st Digit

2nd Digit 3rd Digit

1st Digit

2nd Digit 3rd Digit

## CH1

## CH2

## CH3

## CH4

For product details visit www.texmate.com

Tel: 1-760-598-9899 USA 1-800-839-6283 Thats 1-800-TEXMATE

Page 4

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

ISS5-6 Data Sheet (NZ328)

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.