Dual - Inputs

with Dual Input IDP4 Universal DC volts, mA, 4-20mA Input Module

2 Setpoints per bar Vertical or Horizontal

Configuration

LEOPARD FAMILY

## FL-B202Q

## Leopard Bargraph Meter

## Dual 101 Segment LEDs

## in a 9/64 DIN CASE

MIN-MAX Display

on Right Bar with teseR nottuB hsuP

Left Bar Displays

Single Input and

4 Setpoints using

Leopard Family

I-Series Input

Modules, such as

AC amps, Temperature, Pressure, etc..

Dual Tracking

Setpoints on Right

bar. Adjustable by

External Signal or

Potentiometer

input on CH2.

Left Bar Displays

Single Input on CH1 with Dual Input IDP4 Universal DC volts, mA, 4-20mA

eludoM tupnI

General Features

Two 9 Amp Form C, and two 4 Amp Form A relays available

Auto-sensing AC/DC power supply. For voltages between 85-265

V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

Optional isolated 16 bit analog output. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired span from one bar to the full scale range

24 V DC excitation is available to power external 4/20 mA transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors.

Provision to connect an external programming lockout switch.

Optional NEMA-4 front cover.

UL Listed

Software Features

Utilizes the unique Quickset programming system.

The two 101 segment bargraphs can be independently scaled.

Five user selectable operating modes.

Center zero display mode selectable for one or both bargraphs.

Four programmable setpoints.

Smart dual-bar, dual-input or Single-input bargraph with up to four fully programmable set points and an isolated independenly scalable 16-bit Analog output.

Input Module Compatibility

Dual input modes utilize the FL-B202Q specific IDP4 Universal DC Volts, mA, 4-20mA dual-input

module.

Single Input modes are compatible with the entire LEOPARD FAMILY: More than 38 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Leopard Family of meters.

See www.texmate.com for an up to date listing.

Specifications

Input Specification:........Depends on range & function selected A/D Converter:............14 bit single slope Accuracy:................(0.05% of reading + 1segment) Temp. Coeff.:..............100 ppm/C (Typical) Warm Up Time:............2 minutes Conversion Rate:..........10 conversions per second (Typical) Bargraph Display:.........101 segment 4 vertical dual red bars(std), Dual green bars(optn), one red bar and one green bar(optn) Horizontal bars(optn)

Polarity:..................Selectable center zero Positive Overrange:........Bargraph display flashes Negative Overrange:.......First segment of bargraph display flashes Relay Output:.............Two 4 Amp Form A relays and Two 9 Amp Form C relays

Analog Output:............Isolated 16 bit user scalable mA or V

OIC (mA out)............4-20 mA @ 0 to 500 max loop resistance OIV (volts out)...........0-10 V DC @ 500 or higher resistance

Power Supply:............AC/DC Auto sensing wide range supply PS1 (std)................85-265 VAC, 50-400 Hz / 95-300 VDC @ 4.2W PS2.........................15-48 VAC,50-400 Hz / 10-72 VDC @ 4.2W Operating Temp.:..........0 to 60C Storage Temp:............20C to 70C Relative Humidity:.........95% (non condensing) Case Dimensions:.........9/64 DINBezel: 36x144 mm(1.42x5.69) Depth behind bezel: (4.64") 117.5 mm Plus 10 mm (0.39) for Right-angled connector, or plus 18.3 mm (0.72) for Straight-thru connector

Relay activation is individually selectable to occur above (HI) or

Weight:..................9.5 oz., 12 oz when packed

below (LO) for each setpoint.

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.