### INPUT MODULE

3-pin Input Connector.

Process input (Volts / Current) plus 24 V Excitation.

Excitation Header.

External 24 V available

Signal Type Header.

Voltage / Current

Input Range Header.

Selects 2 V, 5 V, 10 V, 20 V, 200 V,

2 mA, 20 mA, Custom

Interface to

Tiger Meter.

Introducing IP07 The mainstay in process interfacing.

IP07 is a versatile input module presented as a general purpose interface to a wide range of DC voltage or milliamp signal inputs. With an external excitation voltage available to power transducers and onboard selectable headers for interface options, IP07 is the ideal choice between the process inputs and board selectable headers for interface options, IP07 is the ideal choice between the process inputs and your Texmate controller.

p g p g

g g

p p

p p

Input Module

Order Code Suffix

IP07

Signal Type

Choice of DC volts or DC current (header selectable).

Voltage Ranges

Current Ranges

2 V, 5 V, 10 V, 20 V, and 200 V DC (header selectable). (Input Impedance approximately 1 megohm)

2 mA, 20 mA, 1Custom (header selectable). (200 mV drop across shunt resistor)

External Excitation

+24 V DC (150 mA maximum).

Interface

Accuracy

Tiger 320 Series and Leopard range.

0.05% of reading.

Temperature Drift

Typically 50 ppm/C.

Fits Leopard

& Tiger 320 Series

### Connector Pinouts &

### Module Layout

See

Popular IP07 Connection

Configurations

For connection details

Figure 1 IP07 Component Layout

### Technical

### Description

Figure 2 is an IP07 signal flow diagram showing the input signal flow through the signal type, voltage range, and current range headers to the Tiger or Leopard controller for further processing. The signal type header channels the input signal to either the voltage or current range header, which is set to suit the input voltage or current.

For Tiger or Leopard controller supplied +24 V DC excitation, set the excitation header to ON.

If excitation is supplied externally (e.g. from the transducer) set the excitation header to OFF.

Figure 2 IP07 Signal Flow Diagram

### Popular IP07 Connection

### Configurations

Table 1 provides a list of process input signals with and without external excitation and shows the appropriate header positions for each signal type. See diagrams on Page 3.

TABLE 1

POPULAR IP07 CONNECTION CONFIGURATIONS & HEADER POSITIONS

Input

Header Positions

Excitation

Signal Type

Input Range

External Excitation

0-10 V Process Input

0/4-20 mA Process Input

OFF

OFF

VOLTAGE

CURRENT

Controller Supplied Excitation +24 V (150 mA)

Loop Powered Sensors (Current Mode)

0-10 V Process Input

0/4-20 mA Process Input

CURRENT

VOLTAGE

CURRENT

10 V

20 mA

20 mA

10 V

20 mA

External Excitation

0 to 10 V Process Input.

+POS

N/C

+24 V Exc

NEG

+ Supply

+ Signal

External

Supply

Supply

Signal

4 to 20 mA Process Input.

+ Supply

External

Supply

Supply

+ Signal

+POS

+24 V Exc

N/C

NEG

Signal

Controller Supplied Excitation +24 V (150 mA)

2-wire, Loop Powered Sensors (Current Mode).

+POS

+24 V Exc

NEG

N/C

Sensor

3-wire, 0 to 10 V Process Input.

+ Signal

+ Supply

+POS

+24 V Exc

NEG

Signal / Supply

3-wire, 4 to 20 mA Process Input.

+ Signal

+ Supply

+POS

+24 V Exc

NEG

Signal / Supply

### Quick Setup Guide

### Leopard Controller

Calibration

Enter the Calibration Mode and set the [ZEro] and then the [SPAn] settings, while applying a low and then a high signal.

For a full set of calibration and decimal point placement procedures, see your relevant Leopard controller user manual.

### Tiger Controller

Calibration and Input Signal Type Selection Enter the Calibration Mode and then Code 2 to set the following calibration and input signal type settings for CH1:

CAL

000

for CH1 select

111

CODE_2

000

60 Hz Operation:

CODE_2

100

50 Hz Operation:

Code 2 frequency selection applies to all channels

Note, to calibrate the input signal for other engineering units use CH2, CH3, or CH4. These can be viewed

by pressing the

button while in the operational display.

for CH2 select

112

CODE_4

for CH3 select

113

CODE_5

for CH4 select

114

CODE_6

010

010

010

For a full set of calibration and decimal point placement procedures, see your relevant Tiger meter controller manual.

### Customer Configuration Settings:

### IP07 Header Settings

### Calibration Settings

Tel: 1-760-598-9899 USA 1-800-839-6283 Thats 1-800-TEXMATE

Volts

Amps

Display

Input Low

Input High

For product details visit www.texmate.com

Page 4

Texmate, Inc. Tel. (760) 598-9899 www.texmate.com

IP07 (NZ342)

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.