## PL-B101D40

## Leopard Bargraph Meter

## 101 LED Segments

## in a 3/32 DIN Case

LEOPARD FAMILY

Red, 101 segment bargraph, with a 4-digit LED digital display for monitoring, measurement, and control applications, mounted in a 24x144 case.

General Features

External transmitters or signal conditioners can be eliminated

by direct connection of the sensor output to more than

38 Plug-in Input Signal Conditioners that include:

AC/DC Current

Pressure

Resistance

AC/DC Voltage

Process

Temperature

Load Cell

Prototype

4 to 20 mA

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors such as Load Cells and Pressure Transducers.

A red, 101 segment high brightness bargraph.

Red 4-digit LED display with a range of 1999 to 9999

(12000 counts).

Front panel LED annunciators provide indication of setpoint status.

Two 9 Amp Form C, and two 4 Amp Form A relays available.

Auto-sensing AC/DC power supply. For voltages between 85-265 V AC/95-300 V DC (PS1).

Provision to connect an external programming lockout switch.

Provision for external DIM switch to reduce the brightest display setting by 50%.

Automatic intelligent averaging smooths noisy signals, while providing a fast display response to real level changes.

Software Features

The bargraph can display, full scale, any desired portion of the digital reading.

Four programmable setpoints.

Setpoint 1 has delay-onmake and delay-on-break

plus a special pump on pump off mode that creates a Hysteresis Band between SP1 and SP2.

Bargraph center zero function.

Relay activation can be

selected to occur above (hi) or below (Lo) each setpoint.

Digital display blanking.

Decimal point setting.

Four-level brightness control of the bargraph and digital display.

Input Module Compatibility

LEOPARD FAMILY: More than 38 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Leopard Family of meters.

See www.texmate.com for an up to date listing.

LEOPARD

Specifications

Input Specs:..............Depends on Input signal conditioner A/D Converter:..........14 bit single slope Accuracy:..................(0.05% of reading + 2 counts) Temp. Coeff.:............100 ppm/C (Typical) Warm up time:..........2 minutes Conversion Rate:......3 to 16 conversions per second Display:......................4 digit 0.27" Red LED display (std).

Polarity:....................Assumed positive. Displays ve sign.

Decimals:..................User programmable

Positive Overrange:..Bargraph and top segments of digital display flash.

Negative Overrange: First segment of bargraph and bottom

segments of digital display flash.

Display Range:..........1999 to 9999 counts on digital display

Relay Output:............Two 4A form A and two 9A Form C

0 to 101 segments on bargraph

relays.

Power Supply:..........AC/DC Auto sensing wide range supply

85-265 VAC,50-400Hz / 95-300 VDC @4.2W 18-48 VAC, 50-400Hz / 10-72 VDC @4.2W

Operating Temp.:......0 to 50C Storage Temp:..........20C to 70C.

Relative Humidity:....95% (non condensing) Case Dimensions:....3/32 DIN, Bezel: 24x144mm (0.95x5.69), Depth behind bezel 128.6 mm (5.08"), Plus 14 mm (0.55) for connector.

Weight:......................9.5 oz., 12 oz when packed.

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.