## BL-40PSF

## Leopard Panel Meter

## 4 Digit 0.56 LEDs

## in a 1/16 DIN CASE

LEOPARD FAMILY

### An economically smart meter relay with programmable scale factor

### and offset with isolated 4 to 20 mA output retransmission capability

### for measurement and control applications in a 96x48mm case.

### General Features

External transmitters or signal conditioners can be eliminated

by direct connection of the sensor output to more than

38 Plug-in Input Signal Conditioners that include:

AC/DC Current Pressure AC/DC Voltage Process Load Cell

Prototype

Resistance

*Temperature

4 to 20 mA

*See model BL-40H for higher accuracy digitally linearized

thermocouple and RTD

Optional isolated 16 bit analog output. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired digital span from one count to the full scale range of 1999 to 9999 (12000 counts).

Auto-sensing AC/DC power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 15-48 V AC / 10-72 V DC (PS2).

24 V DC excitation is available to power external transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors such as Load Cells and Pressure Transducers.

Standard red or optional green or super bright red 4-digit LED

with display range 1999 to 9999 (12000 counts).

Three annunciator LEDs provide front panel alarm status

indication for up to three setpoints.

One 9 Amp Form C and one 4 Amp Form A relay, or up to

three 4 Amp Form A relays are available.

When analog output is installed, one 9 Amp Form C or two 4

Amp Form A relays can be supported.

Automatic intelligent averaging smooths noisy signals, while providing a fast display response to real level changes.

UL Listed

Software Features

Three-button programming from the front panel

(UP, DOWN and PROGRAM buttons).

Three front panel selectable ranges.

Front panel selectable four-level brightness control of digital dis-

play, and setpoint LEDs.

Three programmable setpoints.

Relay activation can be selected to occur above (HI) or below

(LO) each setpoint.

Hysteresis setting for all three setpoints. Delay on make and

delay on break for SP1 and SP2.

Peak and Valley. View and Reset.

### Input Module Compatibility

LEOPARD FAMILY: More than 38 different Plug-in I-Series Modular Input Signal Conditioners are approved for Texmates Leopard Family of meters.

See www.texmate.com for an up to date listing.

Specifications

Input Specs:..............Depends on input signal conditioner A/D Converter:...........14 bit single slope Accuracy:...................(0.05% of reading + 2 counts) Temp. Coeff.:.............100 ppm/C (Typical) Warm up time:...........2 minutes Conversion Rate:......5 conversions per second (Typical) Display:......................4 digit 0.56" Red LED display (std), 0.56 Red, Green or Super Bright Red (optn). Range 1999 to 9999 counts.

Polarity:......................Assumed positive. Displays negative Decimal Selection:....Front panel button selectable, XXXX Positive Overrange:..Top segments of digital display flash Negative Overrange:.Bottom segments of digital display flash Relay Output:............Three 4 Amp Form A relays or one 9 Amp

Form C, and one 4 Amp Form A relay.

Analog Output:..........Isolated 16 bit user scalable mA or V OIC (mA out)...........4-20 mA @ 0 to 500 max loop resistance OIV (volts out).......... 0-10 V DC @ 500 or higher resistance Power Supply:...........AC/DC Auto sensing wide range supply PS1 (std)................85-265 VAC 50-400Hz / 95-300 VDC @ 2.3W PS2.........................15-48 VAC 50-400Hz / 10-72 VDC @ 2.3W Operating Temp.:.......0 to 50 C Storage Temp:...........20 C to 70 C.

Relative Humidity:....95% (non condensing) Case Dimensions:.....1/16 DIN Bezel 96x24mm

Depth behind bezel 122.2mm (4.83") Plus 12.7mm (0.5) for Right-angled connectors

Weight:.......................7 oz, 9 oz when packed

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.