## FL-B101D40PS

## Leopard Bargraph Meter

## 101 Segment, 4 Digit 0.32 LEDs

## in a 9/64 DIN CASE

LEOPARD FAMILY

General Features

External transmitters or signal conditioners can be eliminated

by direct connection of the sensor output to more than

40 Plug-in Input Signal Conditioners that include:

AC/DC Current

AC/DC Voltage

Load Cell

Pressure

Process

Prototype

Optional isolated 16 bit analog output. User or factory scalable to 4 to 20 mA, 0 to 20 mA or 0 to 10 V across any desired digital span from one count to the full scale range of 1999 to

9999 (12000 counts).

Resistance

Temperature

4 to 20 mA

A Programmable Tricolor (Red-Green-Orange) or mono color

(red or green), 101 segment high brightness bargraph.Vertical or optional horizontal format.

Red 4-digit LED display with a range of -1999 to 9999

(12000 counts). Optional green digital display.

Front panel LED annunciators provide indication of setpoint status.

Two 9 Amp Form C, and two 4 Amp Form A relays available

Auto-sensing AC/DC power supply. For voltages between

85-265 V AC / 95-300 V DC (PS1) or 18-48 V AC / 10-72 V DC (PS2).

24 V DC excitation is available to power external 4/20mA transmitters and 5 or 10 V DC excitation is available for resistance bridge type sensors.

Provision to connect an external programming lockout switch.

Provision for external DIM switch to reduce the brightest

display setting by 50%.

Optional NEMA-4 front cover.

Automatic intelligent averaging, smooths noisy signals while providing a fast display response to real level changes.

UL Listed

Software Features

The bargraph can display, full scale, any desired portion of the digital reading.

Setpoint 1 has delay-on-make and delay-on-break plus a special pump on pump off mode that creates a Hysteresis Band between

SP1 and SP2.

Bargraph center zero function.

Four programmable setpoints with adjustable Hysteresis.

Relay activation can be

selected to occur above (hi) or below (Lo) each setpoint.

Digital display blanking.

Decimal point setting.

Four-level brightness control

### This smart Tricolor or Mono-color digital bar-

### graph with programmable scale factor

### has four fully programmable set points for mon-

### itoring, measurement, and control applications.

Input Module Compatibility

LEOPARD FAMILY: More than 38 different Plug-in I-Series Input Signal Conditioners are approved for Texmates Leopard Family of meters.

See www.texmate.com for an up to date listing.

LEOPARD

Specifications

Input Specs:..............Depends on Input signal conditioner A/D Converter:..........14 bit single slope Accuracy:..................(0.05% of reading + 2 counts) Temp. Coeff.:............100 ppm/C (Typical) Warm up time:..........2 minutes Conversion Rate:......10 conversions per second (Typical) Digital Display:..........4 digit 0.31" LED red (std), green (optn)

Range 1999 to 9999 counts.

Bargraph Display:....101 segment 4 red vertical (std),

green or tricolor (optn), horizontal (optn) Polarity:....................Assumed positive. Displays negative Decimal Selection:....Front panel button selectable, XXXX Positive Overrange:..Bargraph and top segments of digital display flash.

Negative Overrange: First segment of bargraph and bottom

Relay Output:............Two 4 Amp Form A relays and Two

segments of digital display flash.

9 Amp Form C relays.

Analog Output:........Isolated 16 bit user scalable mA or V

OIC (mA out)..........4-20 mA @ 0 to 500 max loop resistance OIV (volts out)..........0-10 V DC @ 500 or higher resistance Power Supply:..........AC/DC Auto sensing wide range supply 85-265 VAC,50-400Hz / 95-300 VDC @ 4.2W 18-48 VAC,50-400Hz / 10-72 VDC @ 4.2W

PS1 (std)................

PS2........................

Operating Temp.:......0 to 50C Storage Temp:..........20C to 70C Relative Humidity:....95% (non condensing) Case Dimensions:....9/64 DIN (Bezel 36Wx144Hmm)

Depth behind bezel (5.83") 148mm Plus (0.7) 18mm for connectors

Weight:......................9.5 oz., 12 oz when packed

accessed by the

and adjusted by the

button

button.

### About TexMate

Texmate is an American manufacturer of high durability industrial grade panel meters, bar graphs, and transducers. Texmate's meters are frequently equipped with relays and various signal outputs for industrial automation applications and are known for their extremely long service life.